The file "zImage" includes two files "wifi.tar.bz2" and "wpa_supplicant.tar.bz2",
the user can download the zImage directly into SBC6410 and test the WIFI module.
The test way is below:
Enter into Linux command line, and input below :

[root@EmbedSky /]#cd /sys/bus/sdio/devices
[root@EmbedSky devices]# ls
[1;36mmmc1:0001:10m]
[root@EmbedSky devices]# ping 192.168.0.20  
PING 192.168.0.20 (192.168.0.20): 56 data bytes
64 bytes from 192.168.0.20: seq=0 ttl=64 time=21.165 ms